This release started with the problem of not having a sidetone for remote stations.  This is not the best place to solve the problem, but may help some folks until a better solution comes along.  In order to generate an appropriate sidetone for those (almost everyone) using logging software a level of integration is required.  I chose to work with N1MM as it appears to be the most widely used program.  Read the documentation for details.

I had the code to connect to DX Clusters and send the spots to your radio, so I added a rudimentary form of that into Flex Buttons.  I also added the ability to start up GRiTTY and WSJT by adjusting their INI files based on the radio's DAX settings.  You can also start CW Skimmer and it's spots will show up on the radio along with DX Cluster spots. If you're using a logging program that supports them it's probably better to start them from the logging program.

Thanks to Len KD0RC, I think I have the CW Speed issues resolved.  That should all work a little smoother with this version.

There are so many variations out there in how people are configured with radios, remoteness and auxilliary software that I can't check them all.  I try to test with configurations that I can setup here, but I don't come close to full coverage.  That said, if you find a problem let me know and I'll do my best to figure out a solution.
